\Velocity\... contains the velocity data collected with a single point ADV, and a profiling-ADV. The two files, 'x_measurement_locations.txt' and 'y_measurement_locations.txt' contain matrices with the coordinates for the 10 equally spaced locations of velocity measurements in each of the 15 cross sections.

There are 15 folders from XS2 to XS16. Each folder contains velocity profiles through the water column (z) at a fixed location in the local flume coordinate system (x,y). 

Each folder contains 12 .txt files with velocity measurements spaced across the XS. sta_LW and sta_RW contain measurements taken as close to the left and right walls as possible. In some instances, flow was too shallow near the walls to take measurements.

Each .txt file contains the following columns: 
station (m) - the distance from an arbitrary point across the channel from the left bank, looking upstream. Note: the left bank (looking upstream) does not necessarily have a station value of 0 (m).
z (m) - Elevation in the flume coordinate system at which the velocity measurement was taken.
u (m/s) - Positive velocity values point downstream parallel to the channel centerline at each cross section. Values were averaged over 30 second sample at 100hz.
v (m/s) - Positive values point to the right bank looking upstream. Values were averaged over 30 second sample at 100hz.
w (m/s) - Positive values point up.Values were averaged over 30 second sample at 100hz.


