This record contains tables with location and measurements data from hydrologic (streamflow) work performed in Summer 2012 by S.R.Fassnacht, Niah B.H. Venable, Odgarav Jigjidsuren and Sukhbaatar Jamiyankhuyag. NBHV 23 Oct 2013.

The hydrologic data were collected either by current meter and wading (Tuin_Q1-Q09) or float method (Tuin_Q10-Q12, QBogD, QAbvOrog) techniques. 

The record contains 3 folders, 2 tables, a codebook, and a set of photos:
o hydro_fieldwork_Q_summary.tsv: a table with a row for each  measurement, and a column for the site name and one for the corresponding calculated Q value. 
o hydro_fieldwork_metadata.tsv: a table containing location and weather data about the measurements for each tuin
o wading_data/: contains tables and metadata for the hydrology data collected by wading
o float_data/:contains tables and metadata for the hydrology data collected by float
o location_metadata/: tables containing information about met and gage locations
o Field_Photos_2012_07_08.pdf has selected field photos keyed to the hydrologic and hydraulic (https://hdl.handle.net/10217/201560) field data .
o Data_dictionary.csv contains a list of variable names, definitions and possible values.
